**R406.2 (N1106.2) Mandatory Requirements:** Compliance with this section requires that the provisions identified in Sections R401 through R404 labeled as 'mandatory' and section R403.5.3 be met. The building thermal envelope shall be greater than or equal to levels of efficiency and Solar Heat Gain Coefficient in Tables R402.1.1 or R402.1.3 of the 2009 International Energy Conservation Code.

 Exception: Supply and return ducts not completely inside the building thermal envelope shall be insulated to a minimum of R-6.

This amendment reflects errata to version 1 of the 2015 IECC/IRC.